(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 73)
    (tracks 629)
    (zones 0)
    (modules 37)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 1.3)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(JP1-Pad1)")
  (net 4 RAW)
  (net 5 TX)
  (net 6 RX)
  (net 7 D3)
  (net 8 D5)
  (net 9 D6)
  (net 10 MOSI)
  (net 11 MISO)
  (net 12 SCK)
  (net 13 A0)
  (net 14 A1)
  (net 15 A4)
  (net 16 A5)
  (net 17 Reset)
  (net 18 A3)
  (net 19 Flash_CS)
  (net 20 VCC)
  (net 21 D2/IRQ)
  (net 22 CS)
  (net 23 CSN)
  (net 24 "Net-(JP3-Pad2)")
  (net 25 "Net-(JP4-Pad1)")
  (net 26 "Net-(IC1-Pad28)")
  (net 27 "Net-(IC1-Pad27)")
  (net 28 "Net-(IC1-Pad7)")
  (net 29 "Net-(IC1-Pad10)")
  (net 30 "Net-(IC1-Pad19)")
  (net 31 "Net-(IC1-Pad22)")
  (net 32 "Net-(P3-Pad1)")
  (net 33 "Net-(P6-Pad1)")
  (net 34 "Net-(P6-Pad2)")
  (net 35 "Net-(P6-Pad3)")
  (net 36 "Net-(P6-Pad4)")
  (net 37 "Net-(P7-Pad1)")
  (net 38 "Net-(P7-Pad2)")
  (net 39 "Net-(P7-Pad3)")
  (net 40 "Net-(P7-Pad4)")
  (net 41 "Net-(P8-Pad1)")
  (net 42 "Net-(P8-Pad2)")
  (net 43 "Net-(P9-Pad1)")
  (net 44 "Net-(P9-Pad2)")
  (net 45 "Net-(P10-Pad1)")
  (net 46 "Net-(P11-Pad1)")
  (net 47 "Net-(P12-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net CS)
    (add_net D2/IRQ)
    (add_net D3)
    (add_net D5)
    (add_net D6)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net RX)
    (add_net Reset)
    (add_net TX)
  )
  (net_class Big ""
    (clearance 0.3)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(JP1-Pad1)")
    (add_net VCC)
  )
  (net_class RAW ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net RAW)
  )
  (net_class SPI ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CSN)
    (add_net Flash_CS)
    (add_net MISO)
    (add_net MOSI)
    (add_net SCK)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AC3D102)
    (at 164.84 78.87 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P7 (at 0.1 8.93 90) (layer F.SilkS) hide)
    (fp_text value X7 (at 0.02 8.93 90) (layer F.Fab))
    (fp_text user %R (at 0.1 8.62 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P7-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:MYSX_2.4 (layer F.Cu) (tedit 5A95B4A4)
    (at 127.254 108.9152 90)
    (descr "Through hole pin header")
    (tags "pin header MYSX 2.4")
    (fp_text reference P2 (at -0.4572 -1.27 90) (layer F.SilkS) hide)
    (fp_text value MYSX_2.4 (at 1.23698 0.12446 180) (layer F.SilkS) hide)
    (fp_text user 2.4 (at -1.1176 -1.2446 270) (layer Cmts.User) hide)
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 A1))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 A0))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 A4))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 A5))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 D6))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 D5))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 D2/IRQ))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 D3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(JP3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 TX))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 RX))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 Reset))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08.wrl
      (offset (xyz 1.269999980926514 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 5AC3D137)
    (at 134.5692 79.9084 270)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference IC1 (at 2.56286 3.25882) (layer F.SilkS) hide)
    (fp_text value ArduinoProMini (at 14.95552 3.41376) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad28)"))
    (pad 27 thru_hole oval (at 7.62 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad27)"))
    (pad 1 thru_hole rect (at -13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 TX))
    (pad 2 thru_hole oval (at -11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 RX))
    (pad 3 thru_hole oval (at -8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 Reset))
    (pad 4 thru_hole oval (at -6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 D2/IRQ))
    (pad 6 thru_hole oval (at -1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 D3))
    (pad 7 thru_hole oval (at 1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole oval (at 3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 D5))
    (pad 9 thru_hole oval (at 6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 D6))
    (pad 10 thru_hole oval (at 8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 Flash_CS))
    (pad 12 thru_hole oval (at 13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 CS))
    (pad 13 thru_hole oval (at 13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 CSN))
    (pad 14 thru_hole oval (at 11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 A0))
    (pad 18 thru_hole oval (at 1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 A1))
    (pad 19 thru_hole oval (at -1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(IC1-Pad19)"))
    (pad 20 thru_hole oval (at -3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 A3))
    (pad 21 thru_hole oval (at -6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 VCC))
    (pad 22 thru_hole oval (at -8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(IC1-Pad22)"))
    (pad 23 thru_hole oval (at -11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 RAW))
    (pad 25 thru_hole oval (at -2.54 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 A4))
    (pad 26 thru_hole oval (at -5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 A5))
    (pad 30 thru_hole oval (at 13.97 -5.08 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole oval (at 13.97 -2.54 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole oval (at 13.97 0 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (offset (xyz -3.809999942779541 5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (offset (xyz 13.96999979019165 2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (offset (xyz 0 7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (offset (xyz 0 -7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (offset (xyz 6.349999904632568 5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl
      (offset (xyz -1.269999980926514 0 12.19199981689453))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (offset (xyz 1.269999980926514 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (offset (xyz 0 -7.619999885559082 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (offset (xyz 0 7.619999885559082 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (offset (xyz 13.96999979019165 2.539999961853027 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 6.349999904632568 5.079999923706055 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz -3.809999942779541 5.079999923706055 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (offset (xyz -7.619999885559082 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (offset (xyz 13.96999979019165 -4.444999933242798 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (offset (xyz -16.50999975204468 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (offset (xyz -7.619999885559082 -1.269999980926514 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (offset (xyz 13.96999979019165 -3.174999952316284 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (offset (xyz -7.619999885559082 1.269999980926514 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (offset (xyz -8.889999866485596 3.809999942779541 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (offset (xyz -8.889999866485596 -3.809999942779541 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (offset (xyz -10.15999984741211 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (offset (xyz -12.69999980926514 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A931A7B)
    (at 150.7744 64.03848)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference P3 (at -0.04572 0.13208) (layer F.SilkS) hide)
    (fp_text value Mount_Hole (at 0.01016 0.00508) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P3-Pad1)"))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A903C0F)
    (at 132.1689 102.0953)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -0.7366 1.397) (layer F.SilkS) hide)
    (fp_text value R (at -0.3048 1.397 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 D5))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A95A8BA)
    (at 165.1 87.09)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 1.01918 0.99212) (layer F.SilkS) hide)
    (fp_text value 1M (at 6.57924 0.99466) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AC3D0B3)
    (at 155.2556 93.6498 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 3.79032 -2.6416 180) (layer F.SilkS) hide)
    (fp_text value C (at 1.2808 -0.0254 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AC3D0BE)
    (at 158.4706 93.6498)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0.01524 0.00508) (layer F.SilkS) hide)
    (fp_text value 10uF (at 1.28016 -0.00508 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5AB4094C)
    (at 149.352 99.568 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at -0.82804 1.25984 180) (layer F.SilkS) hide)
    (fp_text value REG (at 0.0254 1.2446 180) (layer F.Fab) hide)
    (fp_text user "" (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5AB40946)
    (at 145.7579 99.5426 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at -0.7366 1.27 180) (layer F.SilkS) hide)
    (fp_text value BAT (at 0.0254 1.27 180) (layer F.Fab) hide)
    (fp_text user %R (at -0.0127 0.0254 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5AB409BF)
    (at 140.65 98.19 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at -10.5664 0.7112 90) (layer F.SilkS) hide)
    (fp_text value RAW (at -10.0584 -0.9144 270) (layer F.Fab) hide)
    (fp_text user "" (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 RAW))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5AC3D11C)
    (at 166.39 100.28 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference U1 (at 1.54312 -1.48492 180) (layer F.SilkS) hide)
    (fp_text value DC/DCBooster (at 1.53804 0.40992 180) (layer F.Fab) hide)
    (fp_text user %R (at -0.00628 2.55368 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AC3D150)
    (at 164.77 108.49)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.48338 -2.20912 180) (layer F.SilkS) hide)
    (fp_text value 0,1uF (at 0.3988 1.57548) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0EB)
    (at 164.85 68.71 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at -0.04 10.36 90) (layer F.SilkS) hide)
    (fp_text value X4 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at -0.12 11.72 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0F1)
    (at 164.84 71.2 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at -0.15 10.3 90) (layer F.SilkS) hide)
    (fp_text value X5 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at -0.14 11.75 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0FF)
    (at 164.83 76.26 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P7 (at 0.04 8.98 90) (layer F.SilkS) hide)
    (fp_text value X7 (at 0.04 8.82 90) (layer F.Fab))
    (fp_text user %R (at 0.08 8.94 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0F7)
    (at 164.83 73.74 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P6 (at -0.02 10.4 90) (layer F.SilkS) hide)
    (fp_text value X6 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at -0.02 11.63 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P6-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0E0)
    (at 164.85 63.67 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P9 (at 0.4664 13.1588 90) (layer F.SilkS) hide)
    (fp_text value X9 (at 0.16 10.18 90) (layer F.Fab))
    (fp_text user %R (at 0.12 11.58 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P9-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ASKicadLib:3_block_Screw_Terminal (layer F.Cu) (tedit 5A903C2E)
    (at 155.178 106.6292 180)
    (fp_text reference P1 (at 0.0094 -0.0254 180) (layer F.SilkS) hide)
    (fp_text value Power (at 0.0094 0 180) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 4.81 0 180) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 RAW))
    (pad 1 thru_hole circle (at -5 0 180) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A95A8B2)
    (at 165.1 83.88)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.00394 1.0068) (layer F.SilkS) hide)
    (fp_text value 470k (at 6.32524 0.9941) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5A931497)
    (at 133.37376 71.94912 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.79 0 270) (layer B.SilkS))
    (fp_text value 0,1uF (at -0.0245 -0.05988 270) (layer B.Fab))
    (fp_text user %R (at 5.2206 -27.49188 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5AC3EAAE)
    (at 137.00376 69.43912 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.972 0.062) (layer B.SilkS))
    (fp_text value 10k (at -0.0006 0.00886 270) (layer B.Fab))
    (fp_text user "" (at 31.62088 13.29376 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 A3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 5AC3EAAC)
    (at 132.64376 68.84912 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 1.891 -1.277 180) (layer B.SilkS))
    (fp_text value ATSHA204A (at 0.00496 -0.04838 270) (layer B.Fab))
    (fp_text user "" (at 9.13376 -30.45088 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 A3))
    (pad 2 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AC3D0C8)
    (at 170.03 91.54 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 3.78316 -2.59256 180) (layer F.SilkS) hide)
    (fp_text value C (at -0.05732 -0.03224) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A0))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5A931682)
    (at 133.38376 75.91912 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.11 0.03 270) (layer B.SilkS))
    (fp_text value 0,1uF (at -0.02974 -0.02434 180) (layer B.Fab))
    (fp_text user %R (at 1.92606 -0.6441 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A931B02)
    (at 133.35634 87.97798 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.11 0.07 90) (layer B.SilkS))
    (fp_text value 10k (at 0.0292 0.02286 270) (layer B.Fab))
    (fp_text user %R (at 6.41476 -2.10566 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 Flash_CS))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 5A9314B4)
    (at 133.30428 80.72122 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0.98 -1.465 180) (layer B.SilkS))
    (fp_text value AT25DF512C (at 1.6151 0.98644 180) (layer B.Fab))
    (fp_text user %R (at 1.65356 -2.09804 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 Flash_CS))
    (pad 2 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 MISO))
    (pad 3 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 MOSI))
    (pad 6 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 SCK))
    (pad 7 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A903C24)
    (at 128.2192 99.4664)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference P3 (at 0 0.0762) (layer F.SilkS) hide)
    (fp_text value Mount_Hole (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A903C5A)
    (at 171.68622 108.67644)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference P10 (at 0.05378 0.13356) (layer F.SilkS) hide)
    (fp_text value Mount_Hole (at -0.0193 0.0215) (layer F.Fab))
    (fp_text user %R (at -0.02622 0.09356) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 45 "Net-(P10-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A931A85)
    (at 172.03 64.1)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference P11 (at 0.01436 0.09088) (layer F.SilkS) hide)
    (fp_text value Mount_Hole (at -0.00088 0.01468) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 46 "Net-(P11-Pad1)"))
  )
  (module ASKicadLib:TO-92_LE33_Andreas (layer F.Cu) (tedit 5AC3D1E3)
    (at 157.5816 99.5172 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 3.69316 -2.50952 180) (layer F.SilkS) hide)
    (fp_text value LE33 (at 1.26492 -1.30048 180) (layer F.Fab))
    (fp_text user %R (at 1.25984 -1.27508 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.25 -1.25 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.625 0.45 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 20 VCC))
    (pad 1 thru_hole circle (at -0.1 0.475 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5AC3D0E5)
    (at 164.84 66.19 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P8 (at 1.23586 13.48932 90) (layer F.SilkS) hide)
    (fp_text value X9 (at 0.4891 10.46672 90) (layer F.Fab))
    (fp_text user %R (at 0.07508 11.71386 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P8-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AC3D112)
    (at 149.28 87.28)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C6 (at 2.02 -1.62) (layer F.SilkS))
    (fp_text value 4,7uF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5AC3EAA5)
    (at 132.11 98.18)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference JP4 (at 3.4417 -1.09728) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 2.97 1.19) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(JP4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D2/IRQ))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A95BBF5)
    (at 148.49 92.63)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference P12 (at 0.04318 -0.0254) (layer F.SilkS) hide)
    (fp_text value Mount_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 47 "Net-(P12-Pad1)"))
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 5AB15C5B)
    (at 146.746 82.374 180)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U3 (at -2.574 3.054 180) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at -8.382 7.112 180) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(JP4-Pad1)"))
    (pad 5 thru_hole oval (at -6.604 1.524 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 CS))
    (pad 4 thru_hole oval (at -4.064 4.064 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (offset (xyz -5.333999919891357 -2.79399995803833 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (offset (xyz -5.333999919891357 -2.79399995803833 11.22679983139038))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (offset (xyz -7.619999885559082 -14.40179978370666 12.06499981880188))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (offset (xyz -5.58799991607666 -12.95399980545044 12.92859980583191))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (offset (xyz -12.69999980926514 -12.06499981880188 12.95399980545044))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module graphicslogo:OpenSourceLogo_1000x1000_neg (layer F.Cu) (tedit 0)
    (at 156.972 70.104)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_line (start 124.44 61.61) (end 124.77 61.61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.44 111.54) (end 124.44 61.61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.66 111.54) (end 124.44 111.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.65 111.53) (end 124.64 111.53) (layer Edge.Cuts) (width 0.15))
  (gr_text Nrf24l01+ (at 159.004 83.058) (layer F.SilkS))
  (gr_text 4,7uF (at 150.48 90.87) (layer F.SilkS))
  (gr_text "IRQ (Radio)" (at 133.38 96.11) (layer F.SilkS))
  (gr_text "MysX 2,4" (at 125.32868 107.7468 90) (layer F.SilkS))
  (gr_text Arduino (at 134.94512 88.9) (layer F.SilkS))
  (gr_text "Ext. Flash" (at 133.57376 73.83912) (layer B.SilkS))
  (gr_text Signing (at 134.22376 66.11112) (layer B.SilkS))
  (gr_text "-Optional-\n" (at 134.09676 64.54912) (layer B.SilkS))
  (gr_text 10uF (at 159.67 90.19) (layer F.SilkS))
  (gr_text 0,1uF (at 154.1 90.19) (layer F.SilkS))
  (gr_text "Voltage \nReg." (at 160.20034 102.16642 90) (layer F.SilkS))
  (gr_text 0,1uF (at 166.05 105.07) (layer F.SilkS))
  (gr_text "0,1uF\n" (at 173.18 91.53 90) (layer F.SilkS))
  (gr_text "1MΩ\n" (at 168.94 87.12) (layer F.SilkS))
  (gr_text "470kΩ\n" (at 168.91 83.9) (layer F.SilkS))
  (gr_text "D5 Resistor" (at 137.27176 101.50348) (layer F.SilkS))
  (gr_text "Out Gnd In" (at 168.79 102.49) (layer F.SilkS))
  (gr_text GND (at 162.83 71.4 90) (layer F.SilkS))
  (gr_text VCC (at 162.91 68.69 90) (layer F.SilkS))
  (gr_text "Vin Gnd Vout" (at 156.57322 97.0788) (layer F.SilkS))
  (gr_text "BAT REG  " (at 148.336 94.8309) (layer F.SilkS))
  (gr_text "RAW    GND    REG\n" (at 155.22 109.69) (layer F.SilkS))
  (gr_text "Pro Mini" (at 135.01624 90.4621) (layer F.SilkS))
  (gr_text openhardware.io (at 134.5018 72.659) (layer F.SilkS))
  (gr_text openhardware.io (at 157.04 75.76) (layer F.SilkS))
  (gr_text "by sundberg84" (at 157 65.74) (layer F.SilkS))
  (gr_text "Easy PCB" (at 156.93 64.27) (layer F.SilkS))
  (gr_text "Licensed under \nCERN OHL v.1.2" (at 134.6518 70.549) (layer F.SilkS))
  (gr_text "NRF24 Edition" (at 134.4518 68.299) (layer F.SilkS))
  (gr_text "Rev 10" (at 134.747 66.3194) (layer F.SilkS))
  (gr_text "Easy PCB" (at 134.4918 64.099) (layer F.SilkS))
  (gr_text "RAW (MysX)" (at 139.42 96.15) (layer F.SilkS))
  (gr_text "3,3 GND RX GND D2 D6 A4 A1" (at 135.67156 104.3432) (layer F.SilkS))
  (gr_text "Raw V+ TX RST D3 D5  A5 A0\n" (at 135.83412 110.91418) (layer F.SilkS))
  (gr_text "Bat. measurer" (at 168.62 81.84) (layer F.SilkS))
  (gr_text Temp/Hum (at 137.27176 102.6668) (layer F.SilkS))
  (gr_text Booster (at 168.88 96.55) (layer F.SilkS))
  (gr_line (start 174.51 111.54) (end 124.64 111.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.51 61.61) (end 174.51 111.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.55 61.61) (end 174.51 61.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.23 111.51) (xy 175.0298 111.5281) (xy 175.0298 60.9567) (xy 124.29 61.45) (xy 124.2 111.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 61.43) (xy 175.209098 60.639036) (xy 175.30872 112.03736) (xy 124.21 111.53) (xy 124.23 61.52)
      )
    )
  )
)
