(kicad_pcb (version 20160815) (host pcbnew no-vcs-found-7406~56~ubuntu16.10.1)
  (general
    (links 201)
    (no_connects 0)
    (area 115.720475 54.7629 173.201046 130.929001)
    (thickness 1.6)
    (drawings 12)
    (tracks 1782)
    (zones 0)
    (modules 76)
    (nets 84)
  )
  (page A4)
  (title_block
    (title "Sensebender GW module")
    (company "Mysensors Org")
    (comment 1 "Created by Thomas Mørch ")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x230f8_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(C14-Pad2)")
  (net 4 /D-)
  (net 5 /D+)
  (net 6 /SWCLK)
  (net 7 /SWDIO)
  (net 8 /MISO)
  (net 9 /NET_RST)
  (net 10 /SCK)
  (net 11 /MOSI)
  (net 12 "Net-(U4-Pad8)")
  (net 13 "Net-(U4-Pad9)")
  (net 14 "Net-(U4-Pad10)")
  (net 15 "Net-(U7-Pad3)")
  (net 16 "Net-(U7-Pad4)")
  (net 17 "Net-(U7-Pad5)")
  (net 18 "Net-(U7-Pad6)")
  (net 19 "Net-(U7-Pad16)")
  (net 20 "Net-(U11-Pad4)")
  (net 21 /NET_MISO)
  (net 22 /NET_MOSI)
  (net 23 /NET_SCK)
  (net 24 /NET_SS)
  (net 25 "Net-(C17-Pad2)")
  (net 26 /CS_RFM)
  (net 27 /CS_NRF)
  (net 28 "Net-(C18-Pad2)")
  (net 29 "Net-(C19-Pad2)")
  (net 30 /SECURITY)
  (net 31 "Net-(P4-Pad6)")
  (net 32 "Net-(P4-Pad8)")
  (net 33 /IRQ_NRF)
  (net 34 /IRQ_RFM)
  (net 35 /CE_NRF)
  (net 36 /Reset)
  (net 37 /LED1)
  (net 38 /LED2)
  (net 39 /LED3)
  (net 40 "Net-(R8-Pad2)")
  (net 41 "Net-(D1-Pad2)")
  (net 42 "Net-(D2-Pad2)")
  (net 43 "Net-(D3-Pad2)")
  (net 44 "Net-(D4-Pad2)")
  (net 45 /LED4)
  (net 46 "Net-(FB3-Pad2)")
  (net 47 "Net-(U11-Pad8)")
  (net 48 "Net-(U11-Pad9)")
  (net 49 /D14_CS)
  (net 50 /D13_SCK)
  (net 51 /D12_MISO)
  (net 52 /D11_MOSI)
  (net 53 /D8_SDA)
  (net 54 /D7_SCL)
  (net 55 /D6_PWM)
  (net 56 /D5_PWM)
  (net 57 /D4_INT)
  (net 58 /D3_INT)
  (net 59 /D1_DFM)
  (net 60 /D2_DTM)
  (net 61 +3.3VP)
  (net 62 "Net-(CON1-Pad1)")
  (net 63 "Net-(CON1-Pad8)")
  (net 64 /CS_SDCARD)
  (net 65 /SDCARD_DET)
  (net 66 +3V3)
  (net 67 /BAT_DET)
  (net 68 /LED5)
  (net 69 /INCL_SW)
  (net 70 "Net-(D5-Pad2)")
  (net 71 /RESET_RFM)
  (net 72 /RFM_DIO5)
  (net 73 /SWC1)
  (net 74 /SWC3)
  (net 75 /SWC2)
  (net 76 /LEGACY_ID)
  (net 77 "Net-(C20-Pad1)")
  (net 78 /RST)
  (net 79 /D10_A4)
  (net 80 /D9_A3)
  (net 81 /A5)
  (net 82 /A6)
  (net 83 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /A5)
    (add_net /A6)
    (add_net /BAT_DET)
    (add_net /CE_NRF)
    (add_net /CS_NRF)
    (add_net /CS_RFM)
    (add_net /CS_SDCARD)
    (add_net /D+)
    (add_net /D-)
    (add_net /D10_A4)
    (add_net /D11_MOSI)
    (add_net /D12_MISO)
    (add_net /D13_SCK)
    (add_net /D14_CS)
    (add_net /D1_DFM)
    (add_net /D2_DTM)
    (add_net /D3_INT)
    (add_net /D4_INT)
    (add_net /D5_PWM)
    (add_net /D6_PWM)
    (add_net /D7_SCL)
    (add_net /D8_SDA)
    (add_net /D9_A3)
    (add_net /INCL_SW)
    (add_net /IRQ_NRF)
    (add_net /IRQ_RFM)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LED3)
    (add_net /LED4)
    (add_net /LED5)
    (add_net /LEGACY_ID)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NET_MISO)
    (add_net /NET_MOSI)
    (add_net /NET_RST)
    (add_net /NET_SCK)
    (add_net /NET_SS)
    (add_net /RESET_RFM)
    (add_net /RFM_DIO5)
    (add_net /RST)
    (add_net /Reset)
    (add_net /SCK)
    (add_net /SDCARD_DET)
    (add_net /SECURITY)
    (add_net /SWC1)
    (add_net /SWC2)
    (add_net /SWC3)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad8)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(FB3-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U11-Pad8)")
    (add_net "Net-(U11-Pad9)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U7-Pad16)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
  )
  (net_class ANT ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
  )
  (net_class avcc ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net "Net-(C20-Pad1)")
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.635)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 583DDC7F)
    (at 138.50108 98.3488 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0.00504 -1.26492 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C20-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 583DDC79)
    (at 138.42728 97.05848 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB2 (at -0.02304 1.12268 180) (layer F.SilkS))
    (fp_text value "470R EMI" (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C20-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD (layer B.Cu) (tedit 577A9685)
    (at 144.399 88.773 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U7 (at 0.254 1.778 90) (layer B.SilkS))
    (fp_text value RFM69HW (at 6.0452 -7.7597 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 71 /RESET_RFM))
    (pad 2 smd rect (at -1 -2 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 34 /IRQ_RFM))
    (pad 3 smd rect (at -1 -4 90) (size 2.2 1.2) (layers Dwgs.User)
      (net 15 "Net-(U7-Pad3)"))
    (pad 4 smd rect (at -1 -6 90) (size 2.2 1.2) (layers Dwgs.User)
      (net 16 "Net-(U7-Pad4)"))
    (pad 5 smd rect (at -1 -8 90) (size 2.2 1.2) (layers Dwgs.User)
      (net 17 "Net-(U7-Pad5)"))
    (pad 6 smd rect (at -1 -10 90) (size 2.2 1.2) (layers Dwgs.User)
      (net 18 "Net-(U7-Pad6)"))
    (pad 7 smd rect (at -1 -12 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 72 /RFM_DIO5))
    (pad 8 smd rect (at -1 -14 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 66 +3V3))
    (pad 9 smd rect (at 17.9 -14 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 17.9 -12 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(P1-Pad1)"))
    (pad 11 smd rect (at 17.9 -10 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 17.9 -8 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCK))
    (pad 13 smd rect (at 17.9 -6 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 /MISO))
    (pad 14 smd rect (at 17.9 -4 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 /MOSI))
    (pad 15 smd rect (at 17.9 -2 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 26 /CS_RFM))
    (pad 16 smd rect (at 17.9 0 90) (size 2.2 1.2) (layers Dwgs.User)
      (net 19 "Net-(U7-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89C7)
    (at 128.8288 83.6524 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at -0.93476 1.4478) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 /RST))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 583C8AA0)
    (at 140.589 84.328 90)
    (descr "64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (clearance 0.1524)
    (attr smd)
    (fp_text reference U2 (at 0.16764 -0.40132 180) (layer F.SilkS))
    (fp_text value ATSAMD21J (at 0 7.45 90) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C19-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 /A5))
    (pad 4 smd rect (at -5.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 /A6))
    (pad 5 smd rect (at -5.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /SWC2))
    (pad 6 smd rect (at -5.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /RFM_DIO5))
    (pad 7 smd rect (at -5.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -5.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C20-Pad1)"))
    (pad 9 smd rect (at -5.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /SWC1))
    (pad 10 smd rect (at -5.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 /SDCARD_DET))
    (pad 11 smd rect (at -5.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 /BAT_DET))
    (pad 12 smd rect (at -5.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 13 smd rect (at -5.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /D5_PWM))
    (pad 14 smd rect (at -5.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /D3_INT))
    (pad 15 smd rect (at -5.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /D6_PWM))
    (pad 16 smd rect (at -5.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /D4_INT))
    (pad 17 smd rect (at -3.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 /D2_DTM))
    (pad 18 smd rect (at -3.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS_NRF))
    (pad 19 smd rect (at -2.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /D1_DFM))
    (pad 20 smd rect (at -2.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /SECURITY))
    (pad 21 smd rect (at -1.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 22 smd rect (at -1.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -0.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /RESET_RFM))
    (pad 24 smd rect (at -0.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /NET_RST))
    (pad 25 smd rect (at 0.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /NET_MOSI))
    (pad 26 smd rect (at 0.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /NET_SCK))
    (pad 27 smd rect (at 1.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /NET_MISO))
    (pad 28 smd rect (at 1.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /NET_SS))
    (pad 29 smd rect (at 2.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /CS_RFM))
    (pad 30 smd rect (at 2.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /IRQ_RFM))
    (pad 31 smd rect (at 3.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /IRQ_NRF))
    (pad 32 smd rect (at 3.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /SWC3))
    (pad 33 smd rect (at 5.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at 5.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 35 smd rect (at 5.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 36 smd rect (at 5.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 37 smd rect (at 5.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /MISO))
    (pad 38 smd rect (at 5.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /LED1))
    (pad 39 smd rect (at 5.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /LED4))
    (pad 40 smd rect (at 5.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /LED5))
    (pad 41 smd rect (at 5.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED2))
    (pad 42 smd rect (at 5.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /LED3))
    (pad 43 smd rect (at 5.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /D8_SDA) (clearance 0.1524))
    (pad 44 smd rect (at 5.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /D7_SCL))
    (pad 45 smd rect (at 5.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /D-))
    (pad 46 smd rect (at 5.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (pad 47 smd rect (at 5.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at 5.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 49 smd rect (at 3.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /D12_MISO))
    (pad 50 smd rect (at 3.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /D14_CS))
    (pad 51 smd rect (at 2.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 /CS_SDCARD))
    (pad 52 smd rect (at 2.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (pad 53 smd rect (at 1.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /CE_NRF))
    (pad 54 smd rect (at 1.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd rect (at 0.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C17-Pad2)"))
    (pad 56 smd rect (at 0.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 57 smd rect (at -0.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /SWCLK))
    (pad 58 smd rect (at -0.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /SWDIO))
    (pad 59 smd rect (at -1.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /D11_MOSI))
    (pad 60 smd rect (at -1.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /D13_SCK))
    (pad 61 smd rect (at -2.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /LEGACY_ID))
    (pad 62 smd rect (at -2.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 /INCL_SW))
    (pad 63 smd rect (at -3.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 /D9_A3))
    (pad 64 smd rect (at -3.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /D10_A4))
    (model Housings_QFP.3dshapes/TQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:via-0.6mm (layer F.Cu) (tedit 577A9894)
    (at 136.2 89.4)
    (tags "0.3mm drill")
    (fp_text reference REF** (at 0 0) (layer F.Fab) hide)
    (fp_text value via-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23-5 (layer F.Cu) (tedit 583C89D3)
    (at 132.2984 77.0206 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -2.2782 -0.02028 180) (layer F.SilkS))
    (fp_text value AT24CS32-STUM (at -0.05 2.35 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 54 /D7_SCL))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 /D8_SDA))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89ED)
    (at 143.322 73.279)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at -3.241 0) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8AE4)
    (at 121.285 103.8274 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.7432 0.2794 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 /D8_SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8AE7)
    (at 123.3678 103.8274 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 2.7432 -0.254 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 /D7_SCL))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_buttons:TS-021 (layer F.Cu) (tedit 583C8989)
    (at 141.4918 109.6264 180)
    (descr "Xingda TS-021")
    (tags "SPST Button Switch")
    (fp_text reference SW1 (at 0.03048 0.06096 180) (layer F.SilkS))
    (fp_text value Reset (at 0.99568 -2.64668 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.9 0 180) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.9 0 180) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R8-Pad2)"))
    (pad "" smd rect (at -1.85 -2.075 180) (size 1 1.15) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 1.85 2.075 180) (size 1 1.15) (layers F.Cu F.Paste F.Mask))
    (model mysensors.3dshapes/w.lain.3dshapes/switch/smd_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 583C8945)
    (at 148.7424 93.5482 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference BT1 (at 1.8669 3.1242 270) (layer F.SilkS))
    (fp_text value Battery (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /BAT_DET))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 583C8A52)
    (at 129.2352 65.405 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 1.96596 0.09144 270) (layer F.SilkS))
    (fp_text value LED_RED (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 57D99993)
    (at 133.7437 65.405 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -0.7366 -2.6797 90) (layer F.SilkS))
    (fp_text value LED_ORANGE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C89F7)
    (at 130.9878 71.8488 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.5732 0.0254 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED2))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8969)
    (at 146.42596 106.08056 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 1.204 -1.07696 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23 (layer F.Cu) (tedit 583C8A15)
    (at 154.7876 86.0044)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at -0.04064 -2.15392) (layer F.SilkS))
    (fp_text value ATSHA204A (at -3.2766 1.4478 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 30 /SECURITY))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOT-223 (layer F.Cu) (tedit 583C8935)
    (at 146.6088 100.584)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U10 (at 0 -0.762) (layer F.SilkS))
    (fp_text value AMS1117-3.3 (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 56AE413A)
    (at 122.209 67.218)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.Fab))
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 56AE4119)
    (at 164.711 109.6565)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.Fab))
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 56AE4124)
    (at 122.209 109.6565)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.Fab))
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C899F)
    (at 128.3208 91.9328 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -0.08124 -1.15316 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 57D9996F)
    (at 127.7366 65.405 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -0.0254 1.2446 90) (layer F.SilkS))
    (fp_text value LED_BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8A1E)
    (at 157.2514 85.9536 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.09652 1.52908 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89B5)
    (at 131.511 84.2391 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.0152 -1.4351 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89CE)
    (at 135.9052 76.9112 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -1.22432 1.0414 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8A09)
    (at 148.717 85.156 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.06752 0.09144 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C892D)
    (at 140.2334 93.6346 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.4986 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8983)
    (at 147.9296 109.0828 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.855 0.0762 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 136.906 104.14 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.7432 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C894F)
    (at 151.2824 98.4352 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -2.76352 -0.16256 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8954)
    (at 151.1808 104.0384 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -0.82804 1.6256 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8A27)
    (at 143.317 71.8185 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.2868 0.0127 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C88F5)
    (at 140.25372 101.76256 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at -0.0508 1.33096 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8A24)
    (at 143.1925 70.2945 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB1 (at 3.3147 0.0127 180) (layer F.SilkS))
    (fp_text value "470R EMI" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8A0D)
    (at 152.2476 86.6902 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.20472 0.01524 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /SECURITY))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C89F3)
    (at 129.3368 71.8488 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.5732 -0.0254 180) (layer F.SilkS))
    (fp_text value 91 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /LED1))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89C3)
    (at 131.8006 82.4738)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -0.06604 -1.21412) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8964)
    (at 140.25372 103.30688 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -1.22428 -0.94742 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89B2)
    (at 132.6388 91.186 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 3.2004 0.0254 90) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C8901)
    (at 136.5504 94.107)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at -0.4826 1.12776) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 57D99984)
    (at 130.7338 65.405 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 1.99644 0.4064 90) (layer F.SilkS))
    (fp_text value LED_GREEN (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C89FA)
    (at 132.6388 71.8488 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.5732 0 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /LED3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89E8)
    (at 146.2024 76.9112)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0.05588 -1.14808) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C897A)
    (at 128.143 109.474 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 1.3208 1.4224 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C897E)
    (at 129.794 109.601 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.7178 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8976)
    (at 131.445 109.601 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.0254 -1.6002 270) (layer F.SilkS))
    (fp_text value 39R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 57D9998C)
    (at 132.2324 65.405 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -0.3048 -2.794 90) (layer F.SilkS))
    (fp_text value LED_YELLOW (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C89FE)
    (at 134.2898 71.8488 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.5732 -0.0254 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /LED4))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8A30)
    (at 147.7264 66.802 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB3 (at 0.0762 1.5494 90) (layer F.SilkS))
    (fp_text value "470R EMI" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(FB3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:Cortex_M_Debug_Connector (layer F.Cu) (tedit 583C8999)
    (at 131.5466 96.9772 180)
    (fp_text reference P4 (at -0.23368 -0.13716 180) (layer F.SilkS))
    (fp_text value Debug (at 3.8862 -0.0508 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 1.905 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at -2.54 -1.995 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /SWDIO))
    (pad 3 smd rect (at -1.27 1.905 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.27 -1.995 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /SWCLK))
    (pad 5 smd rect (at 0 1.905 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0 -1.995 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P4-Pad6)"))
    (pad 8 smd rect (at 1.27 -1.995 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P4-Pad8)"))
    (pad 9 smd rect (at 2.54 1.905 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.54 -1.995 180) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /Reset))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_ftsh/FTSH-105-01-L-DV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:XTAL_3.2x1.5mm (layer F.Cu) (tedit 55B4F766)
    (at 135.7235 92.0623 180)
    (descr "XTAL 3.2 x 1.5mm footprint")
    (tags Xtal)
    (fp_text reference X1 (at -3.02768 0.0508 270) (layer F.SilkS))
    (fp_text value 32768hz (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C18-Pad2)"))
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_smd_5x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.64 0.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 56AE4130)
    (at 164.711 67.318 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005 90) (layer F.Fab))
    (fp_text value MountingHole_3mm (at 1.00076 5.00126 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers))
  )
  (module mysensors_connectors:Micro_USB (layer F.Cu) (tedit 583C8A47)
    (at 141.8526 63.6454 180)
    (fp_text reference U11 (at 0.019 -2.1406 180) (layer F.SilkS))
    (fp_text value MICRO-B_USB (at -0.875 7.925 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -4.25 180) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (pad 4 smd rect (at 0.65 -4.25 180) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U11-Pad4)"))
    (pad 2 smd rect (at -0.65 -4.25 180) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /D-))
    (pad 1 smd trapezoid (at -1.3 -4.25 180) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C14-Pad2)"))
    (pad 5 smd rect (at 1.3 -4.25 180) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.575 -1.15 180) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(FB3-Pad2)"))
    (pad 7 thru_hole oval (at 3.575 -1.15 180) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(FB3-Pad2)"))
    (pad 8 thru_hole oval (at -3.575 -4.6 180) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U11-Pad8)"))
    (pad 9 thru_hole oval (at 3.575 -4.6 180) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U11-Pad9)"))
    (pad "" np_thru_hole circle (at -2 -3.275 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2 -3.275 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_pc/usb_B_micro_smd-2.wrl
      (at (xyz 0 0.03 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583C893E)
    (at 145.288 94.30258 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D6 (at -0.06096 2.13106 180) (layer F.SilkS))
    (fp_text value BAT54 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 67 /BAT_DET))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 577AB9F3)
    (at 130.43408 95.23476)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference W1 (at -1.74752 -0.9652) (layer B.Fab))
    (fp_text value SWDIO (at 0.02032 -1.53924) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 7 /SWDIO))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C8A02)
    (at 135.9916 71.8488 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.5986 0 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 /LED5))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 583C8B4C)
    (at 128.3462 76.5302 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW2 (at 1.11252 1.88468 270) (layer F.SilkS))
    (fp_text value SW_INCL (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /INCL_SW))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 577ABA03)
    (at 127.89408 97.76968)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference W3 (at -0.57404 1.5748) (layer B.Fab))
    (fp_text value RESET (at -1.36144 -0.00508 90) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 36 /Reset))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 577ABA09)
    (at 130.43408 100.30968)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference W2 (at 1.8288 0.44704) (layer B.Fab))
    (fp_text value SWCLK (at 0.01524 1.51384) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 6 /SWCLK))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 577AB9FA)
    (at 130.43408 97.76968)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference W4 (at 1.67132 -1.50368) (layer B.Fab))
    (fp_text value GND (at 2.13868 -1.61036) (layer B.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 577ABA0F)
    (at 132.97408 97.76968 90)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference W5 (at 0.75692 1.7272 180) (layer B.Fab))
    (fp_text value "3v3 cpu" (at -0.00508 1.7272 90) (layer B.SilkS))
    (pad 1 smd circle (at 0 0 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 61 +3.3VP))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56F7C332)
    (at 146.8882 71.1962)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.0762 -1.778) (layer F.Fab) hide)
    (fp_text value USB_PWR_DIS (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:MM027S020R (layer F.Cu) (tedit 56A9296F)
    (at 163.9824 96.266 90)
    (tags "SD Card connector litkconn")
    (fp_text reference CON1 (at -0.1778 0.5842 90) (layer F.SilkS))
    (fp_text value micro_SD_Card_SPI (at 0 -5.3594 90) (layer F.Fab))
    (pad 1 smd rect (at 2.2 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 1.1 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 /CS_SDCARD))
    (pad 3 smd rect (at 0 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 4 smd rect (at -1.1 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 5 smd rect (at -2.2 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 6 smd rect (at -3.3 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.4 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /MISO))
    (pad 8 smd rect (at -5.5 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(CON1-Pad8)"))
    (pad 9 smd rect (at -6.6 -10.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 /SDCARD_DET))
    (pad "" np_thru_hole circle (at 3.05 0 90) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -4.93 0 90) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 10 smd rect (at 7.75 -0.4 90) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -7.75 -10 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 6.85 -10 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -7.75 -0.4 90) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/conn_misc/microsd_socket.wrl
      (at (xyz -0.03 0.13 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 585D97E7)
    (at 132.3848 68.4022 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.01524 4.60756 90) (layer F.SilkS))
    (fp_text value ANT (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P1-Pad1)") (clearance 0.7))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_network:W5100 (layer F.Cu) (tedit 583C8991)
    (at 150.876 110.49 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference U4 (at -4.0005 -1.8288 180) (layer F.SilkS))
    (fp_text value W5100 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.254 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0.254 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at -2.286 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /NET_RST))
    (pad 4 thru_hole oval (at -2.286 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /NET_SS))
    (pad 5 thru_hole oval (at -4.826 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /NET_SCK))
    (pad 6 thru_hole oval (at -4.826 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /NET_MOSI))
    (pad 7 thru_hole oval (at -7.366 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /NET_MISO))
    (pad 8 thru_hole oval (at -7.366 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U4-Pad8)"))
    (pad 9 thru_hole oval (at -9.906 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U4-Pad9)"))
    (pad 10 thru_hole oval (at -9.906 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U4-Pad10)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x05.wrl
      (at (xyz -0.2 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz -0.2 -0.05 0.522))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_network.3dshapes/w5100.wrl
      (at (xyz -0.075 -0.85 0.555))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/conn_pc/rj45-led-rb1-125bag1a.wrl
      (at (xyz -0.28 -1.5 0.53))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 5587F36C)
    (at 135.89 101.854)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U8 (at -1.016 -0.7366) (layer F.SilkS))
    (fp_text value NRF24L01 (at -8.382 7.112) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 8 thru_hole oval (at -9.144 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /IRQ_NRF))
    (pad 5 thru_hole oval (at -6.604 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 6 thru_hole oval (at -6.604 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CE_NRF))
    (pad 4 thru_hole oval (at -4.064 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CS_NRF))
    (pad 1 thru_hole rect (at -1.524 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.524 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C895E)
    (at 139.5222 105.2322)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -1.2065 1.4859) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 583C89BA)
    (at 129.8956 91.9353 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3.1877 0.0127 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:via-0.6mm (layer F.Cu) (tedit 577A988A)
    (at 133.7 89.6)
    (tags "0.3mm drill")
    (fp_text reference REF** (at 0 0) (layer F.Fab) hide)
    (fp_text value via-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer B.Cu) (tedit 577AB9CB)
    (at 151 79.5 270)
    (fp_text reference P7 (at -0.635 3.048 270) (layer Cmts.User) hide)
    (fp_text value SWC1 (at 3.7 0 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.4445 0 270) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 73 /SWC1))
    (pad 1 smd rect (at -0.4445 0 270) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd oval (at 0.762 0 270) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 73 /SWC1))
    (pad 1 smd oval (at -0.762 0 270) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer B.Cu) (tedit 577AC061)
    (at 155 79.5 270)
    (fp_text reference P3 (at -0.635 3.048 270) (layer Cmts.User) hide)
    (fp_text value SWC3 (at 3.685 0.0092 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.4445 0 270) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 74 /SWC3))
    (pad 1 smd rect (at -0.4445 0 270) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd oval (at 0.762 0 270) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 74 /SWC3))
    (pad 1 smd oval (at -0.762 0 270) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer B.Cu) (tedit 577AC069)
    (at 153 79.5 90)
    (fp_text reference P6 (at -0.635 3.048 90) (layer Cmts.User) hide)
    (fp_text value SWC2 (at -3.7104 0.0096 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.4445 0 90) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.4445 0 90) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask)
      (net 75 /SWC2))
    (pad 2 smd oval (at 0.762 0 90) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -0.762 0 90) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (net 75 /SWC2))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 583C890E)
    (at 142.113 96.6392 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -0.69324 -1.25476 270) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /BAT_DET))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:MYSX_2.6 (layer F.Cu) (tedit 583C8A5A)
    (at 121.92 74.93)
    (descr "Through hole pin header")
    (tags "pin header MYSX 2.6")
    (fp_text reference P2 (at 0 -3.302) (layer F.SilkS))
    (fp_text value "MYSX 2.6" (at -1.9812 12.573 90) (layer F.SilkS))
    (fp_text user 2.5 (at 2.54 -3.302) (layer Cmts.User))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D14_CS))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D13_SCK))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D12_MISO))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /D11_MOSI))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 /D10_A4))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 /D9_A3))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /D8_SDA))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /D7_SCL))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /D6_PWM))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /D5_PWM))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /D4_INT))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /D3_INT))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /D1_DFM))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /D2_DTM))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 /RST))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 /LEGACY_ID))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 /A5))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 /A6))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x11.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 583DDC13)
    (at 135.6868 97.11944 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 1.52908 -0.11176) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 +3.3VP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SWCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Cut to disable    ->\npower over USB" (at 156.4386 73.2282) (layer B.SilkS))
  (gr_text + (at 149.4028 95.885) (layer F.SilkS))
  (gr_text - (at 149.4028 88.4174) (layer F.SilkS))
  (gr_text Battery (at 151.4094 92.4306 90) (layer F.SilkS))
  (gr_arc (start 163 108) (end 168.5 108) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124 108) (end 124 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 163 69) (end 163 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124 69) (end 118.5 69) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.5 69) (end 118.5 108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163 63.5) (end 124 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.5 108) (end 168.5 69) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124 113.5) (end 163 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119 64) (xy 168 64) (xy 168 113) (xy 119 113)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.402 112.8395) (xy 118.872 113.0935) (xy 118.872 64.0715) (xy 168.402 64.0715)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.2286))
    (polygon
      (pts
        (xy 131.1 89.1) (xy 131.1 95.4) (xy 136.4 95.4) (xy 136.4 88.9) (xy 131.8 88.9)
        (xy 131.8 88.9)
      )
    )
  )
)
