<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="44.43" y1="1.905" x2="44.43" y2="43.993" width="0" layer="20"/>
<wire x1="44.43" y1="43.993" x2="42.525" y2="45.39" width="0" layer="20" curve="90"/>
<wire x1="42.525" y1="45.39" x2="1.905" y2="45.39" width="0" layer="20"/>
<wire x1="1.905" y1="45.39" x2="0" y2="43.485" width="0" layer="20" curve="90"/>
<wire x1="0" y1="43.485" x2="0" y2="1.905" width="0" layer="20"/>
<wire x1="0" y1="1.905" x2="1.905" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="0" x2="42.525" y2="0" width="0" layer="20"/>
<wire x1="42.525" y1="0" x2="44.43" y2="1.905" width="0" layer="20" curve="90"/>
<text>HIGH VOLTAGE SIDE. Be careful. Risk of death!</text>
<text>RollerShutterNode r1.3
(c) Scalz 2016</text>
<text>N</text>
<text>L</text>
<text>L_FUSE</text>
<text>PWR</text>
<text>UP</text>
<text>DOWN</text>
<wire x1="6.096" y1="2.413" x2="6.096" y2="12.192" width="1.27" layer="46"/>
<wire x1="17.907" y1="2.413" x2="17.907" y2="11.176" width="1.27" layer="46"/>
<wire x1="27.94" y1="1.524" x2="27.94" y2="5.08" width="1.27" layer="46"/>
<wire x1="27.94" y1="5.08" x2="27.94" y2="9.652" width="1.27" layer="46"/>
<wire x1="15.748" y1="14.732" x2="5.588" y2="14.732" width="1.27" layer="46"/>
<wire x1="31.496" y1="9.652" x2="27.94" y2="9.652" width="1.27" layer="46"/>
<wire x1="31.496" y1="9.652" x2="34.036" y2="12.192" width="1.27" layer="46"/>
<wire x1="34.036" y1="12.192" x2="34.036" y2="14.732" width="1.27" layer="46"/>
<wire x1="32.004" y1="5.08" x2="27.94" y2="5.08" width="1.27" layer="46"/>
<wire x1="35.19705" y1="7.554628125" x2="32.06936875" y2="5.061946875" width="1.27" layer="46"/>
<wire x1="35.56" y1="7.62" x2="37.846" y2="7.62" width="1.27" layer="46"/>
<wire x1="37.846" y1="7.62" x2="38.227" y2="7.239" width="1.27" layer="46"/>
<wire x1="38.227" y1="7.239" x2="38.227" y2="2.413" width="1.27" layer="46"/>
<wire x1="38.227" y1="2.413" x2="39.243" y2="2.413" width="1.27" layer="46"/>
<wire x1="11.684" y1="2.413" x2="11.684" y2="14.224" width="1.27" layer="46"/>
<wire x1="34.036" y1="14.732" x2="20.828" y2="14.732" width="1.27" layer="46"/>
<text>Creepage sample</text>
<wire x1="42.164" y1="14.732" x2="34.036" y2="14.732" width="1.27" layer="46"/>
<wire x1="16.637" y1="20.066" x2="11.049" y2="20.066" width="1.27" layer="46"/>
<text>BUTTONS/I2C</text>
<text>AVRSPI</text>
<wire x1="5.08" y1="20.066" x2="1.524" y2="20.066" width="1.27" layer="46"/>
<text>FTDI</text>
<text>OpenHardware.io</text>
<text>ANT</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="0805-CAP">
</package>
<package name="0805-RES">
</package>
<package name="0805-LED">
</package>
<package name="RFM12B-ANTENNA">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="L0805">
</package>
</packages>
</library>
<library name="Connector">
<packages>
<package name="2P-5.0">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-1MM">
<description>Works with part #579 (https://www.sparkfun.com/products/579). Commonly used on GPS modules EM408, EM406 and GP-635T. Also compatible with cable 9123 (https://www.sparkfun.com/products/9123) and cable 574 (https://www.sparkfun.com/products/574).</description>
</package>
<package name="1X05-1MM">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="KMR2">
</package>
</packages>
</library>
<library name="pmo_graphics">
<packages>
<package name="ELECTROCUTION_SMALL">
</package>
<package name="OPENHW_IO_SMALL">
</package>
</packages>
</library>
<library name="rollershutter">
<packages>
<package name="2410">
</package>
<package name="HILINK_HLK-PM01">
</package>
<package name="FUSE_BEL_RST5_5A">
</package>
<package name="MDC3105DMT1">
</package>
<package name="G5Q_SINGLE">
</package>
<package name="RELAY-G5Q">
</package>
<package name="RFM12B-MINPADS">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
<package name="TO92-">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="SOIC127P600X175-8N">
</package>
<package name="SOT95P285X120-5N">
</package>
<package name="VARISTOR_B72207S251K101">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC5" library="rollershutter" package="SOT23" value="ATSHA204A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="rollershutter" package="SOIC127P600X175-8N" value="ACS712_5A">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="31M3133"/>
<attribute name="MPN" value="ACS712ELCTR-20A-T"/>
<attribute name="SUPPLIER" value="Allegro"/>
<attribute name="OC_FARNELL" value="1329624"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="LowPowerLab" package="0805-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="LowPowerLab" package="0805-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="LowPowerLab" package="0805-CAP" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="LowPowerLab" package="0805-CAP" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HILINK" library="rollershutter" package="HILINK_HLK-PM01" value="HILINK_HLK-PM01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="rollershutter" package="SOT95P285X120-5N" value="LM321">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="37K8530"/>
<attribute name="MPN" value="LM321MF"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
<attribute name="OC_FARNELL" value="9779116"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="LowPowerLab" package="0805-RES" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="LowPowerLab" package="0805-RES" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun" package="RESONATOR-SMD" value="8 MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="linear" package="SOT23" value="MCP170x, or other SOT23-3 ldo with same footprint">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="LowPowerLab" package="TQFP32-08" value="ATMega-328">
<attribute name="EAGLEUP" value="TQFP32-08"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="LowPowerLab" package="0805-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="LowPowerLab" package="0805-CAP" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="LowPowerLab" package="0805-CAP" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="LowPowerLab" package="0805-CAP" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="rollershutter" package="VARISTOR_B72207S251K101" value="VARISTOR_B72207S251K101">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="LowPowerLab" package="0805-CAP" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="rollershutter" package="FUSE_BEL_RST5_5A" value="FUSE_BEL_RST5_5A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="LowPowerLab" package="0805-RES" value="10k or 0ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="LowPowerLab" package="0805-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="LowPowerLab" package="0805-RES" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="LowPowerLab" package="0805-RES" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="LowPowerLab" package="0805-LED" value="LED0805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="LowPowerLab" package="0805-RES" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="1n914 type">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="C15" library="LowPowerLab" package="0805-CAP" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="rollershutter" package="MDC3105DMT1" value="MDC3105DMT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RL2" library="rollershutter" package="RELAY-G5Q" value="G5Q-1-EU-5VDC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RL1" library="rollershutter" package="G5Q_SINGLE" value="G5Q-1A-5VDC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="LowPowerLab" package="0805-RES" value="56k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="LowPowerLab" package="0805-RES" value="56k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Discrete" package="L0805" value="or 0ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Discrete" package="L0805" value="or 0ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="Discrete" package="L0805" value="or 0ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="rollershutter" package="TO92-" value="DS1820">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="LowPowerLab" package="0805-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Connector" package="2P-5.0" value="SCREW-TERMINAL-2P-3470110P1">
<attribute name="VALUE"/>
</element>
<element name="J2" library="Connector" package="2P-5.0" value="SCREW-TERMINAL-2P-3470110P1">
<attribute name="VALUE"/>
</element>
<element name="J3" library="Connector" package="2P-5.0" value="SCREW-TERMINAL-2P-3470110P1">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X06-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X05-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="microchip" package="SO-08" value="AT25DF512C-SSHN-B">
<attribute name="OC_NEWARK" value="92C7351"/>
<attribute name="MPN" value="25AA080/SN"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1816072"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="LowPowerLab" package="0805-RES" value="56k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="LowPowerLab" package="0805-CAP" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X06-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="adafruit" package="KMR2" value="SPST_TACT-KMR2"/>
<element name="F2" library="rollershutter" package="2410" value="FUSE_MF2410">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="Discrete" package="L0805" value="or 0ohms">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="LowPowerLab" package="0805-CAP" value="10n(DNP)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="LowPowerLab" package="0805-CAP" value="10n(DNP)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANT" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="RFM69CW" library="rollershutter" package="RFM12B-MINPADS" value="RFM69CW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="pmo_graphics" package="ELECTROCUTION_SMALL" value=""/>
<element name="U$3" library="pmo_graphics" package="ELECTROCUTION_SMALL" value=""/>
<element name="U$5" library="pmo_graphics" package="OPENHW_IO_SMALL" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC5" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="R4" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="RFM69CW" pad="VDD"/>
<contactref element="RFM69CW" pad="VDD"/>
</signal>
<signal name="GND">
<contactref element="IC5" pad="3"/>
<contactref element="HILINK" pad="V-"/>
<contactref element="X1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="21"/>
<contactref element="C5" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="D1" pad="MINUS"/>
<contactref element="C16" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC7" pad="GND1"/>
<contactref element="IC7" pad="GND2"/>
<contactref element="C11" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="IC8" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP6" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="RFM69CW" pad="GND"/>
<contactref element="RFM69CW" pad="GND"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="17"/>
<contactref element="IC2" pad="6"/>
<contactref element="JP5" pad="6"/>
<contactref element="RFM69CW" pad="SCK"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="JP5" pad="3"/>
<contactref element="IC2" pad="2"/>
<contactref element="RFM69CW" pad="SDO"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="5"/>
<contactref element="JP5" pad="5"/>
<contactref element="RFM69CW" pad="SDI"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="A3">
<contactref element="IC5" pad="1"/>
<contactref element="IC1" pad="26"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="FLASH_CSN">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="29"/>
<contactref element="R7" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="2"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="32"/>
<contactref element="RFM69CW" pad="IRQ"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC4" pad="6"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="OUT_ACS">
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="3"/>
<contactref element="RL2" pad="2"/>
</signal>
<signal name="PHASE">
<contactref element="F1" pad="2"/>
<contactref element="V1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="N">
<contactref element="HILINK" pad="AC2"/>
<contactref element="V1" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="RF_CSN">
<contactref element="IC1" pad="14"/>
<contactref element="R14" pad="1"/>
<contactref element="RFM69CW" pad="SEL"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="REL_UPDOWN">
<contactref element="IC7" pad="VIN1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="RELAY_POWER">
<contactref element="IC7" pad="VIN2"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="12_220">
<contactref element="RL1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="X1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="X1" pad="3"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="20"/>
<contactref element="C5" pad="1"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="2"/>
<contactref element="IC8" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="D1_TX">
<contactref element="IC1" pad="31"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="D0_RX">
<contactref element="IC1" pad="30"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="A7">
<contactref element="IC1" pad="22"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="A6">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="A4_SDA">
<contactref element="IC1" pad="27"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="A5_SCL">
<contactref element="IC1" pad="28"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="9"/>
</signal>
<signal name="L">
<contactref element="F1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC4" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC6" pad="3"/>
<contactref element="R10" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D1" pad="PLUS"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R5" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LM_OUT">
<contactref element="IC6" pad="4"/>
<contactref element="R10" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC7" pad="VOUT1"/>
<contactref element="RL2" pad="1"/>
</signal>
<signal name="M_UP">
<contactref element="RL2" pad="4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="M_DOWN">
<contactref element="RL2" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC7" pad="VOUT2"/>
<contactref element="RL1" pad="5"/>
</signal>
<signal name="IN_ACS">
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="RL1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="18"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="L2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="R9" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="A7_ADC">
<contactref element="R8" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$5">
</signal>
<signal name="LED">
<contactref element="R12" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="DTR">
<contactref element="C24" pad="1"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$9">
<contactref element="HILINK" pad="AC1"/>
<contactref element="F2" pad="2"/>
</signal>
<signal name="VCC_ACS">
<contactref element="L4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC4" pad="8"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="HILINK" pad="V+"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="RL2" pad="5"/>
<contactref element="RL1" pad="1" route="any" routetag="G$1.COIL1"/>
</signal>
<signal name="N$13">
<contactref element="RFM69CW" pad="ANT"/>
<contactref element="ANT" pad="P$1"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
